Joystick Assembly (0x48)

3v sda scl ground

You will need:

* X inches of Xmm Stranded Wire
* Wire cutter
* Wire stripper

1. Verify your circuit works on the bread board
2. Cut and strip 8 X” long pieces of the stranded wire
3. Solder the wires to the ADS1115